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The KGN Pillinger BTA places the Break Tank above our EV or AV Booster Set range on a stainless steel frame. With multiple tank sizes and dimensions available this unique design permits installation in even the most size restrictive plant rooms.

Advantages
· Efficient use of floor space
· EV or AV Booster set available
· [image: A large white box with several small white boxes on top of a metal table

AI-generated content may be incorrect.]Bespoke design for custom fit installation
Design
One piece or split horizontal tank seated on a stainless steel frame.

EV:    Single or twin pump configuration                                                                                                                                                                             AV:    Multiple pump configurations 
Applications 
· Commercial properties
· Retail developments 
· Apartment blocks
· Water utilities
· Agricultural 
· Leisure centres
· Single dwellings
· Light industrial units
· Schools & universities
Features
· Stainless steel base frame
· Insulation of tank is 25 mm as standard
· 316L stainless steel pipework as standard
· Range of inlet valves in multiple sizes available
· Individual motor mounted inverter drives on each pump
· Single (EV) or Multiple (AV) BMS volt free contacts available
· A/B air gaps fitted as standard to offer complete protection for potable water mains
· Optional remote telemetry system to send fault signal alert via SMS text or telephone line
· Slow Fill system to prevent water surge following a power cut or if the unit cuts out due to low water level (AV)
· Anti-vibration mounts and flexible connections offered as standard to reduce noise transmission in the building
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