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The KGN Pillinger External CAT 5 Washdown Booster Set is designed to prevent backflow contamination of the mains water supply, while maintaining flow and pressure. The unit is compact, lightweight, and housed in a GRP cabinet. Suitable for external use, the unit also has a built in heater for cold weather protection.

Advantages
• Automatic operation
• Simple to wall or floor mount and install
• Easy access and maintenance
• Suitable for external usage

Design
Single peripheral pump and water storage
tank housed in a GRP cabinet.
1 outlet connection only
5 metre hose limitation

Applications
• Bin store washdown
• Limited boosting applications

Features
• Stand stock item
• Duty: 0.25 l/s @ 2.2 bar (mid curve)
• Lightweight GRP Kiosk
• Break Tank: 18 litre (4 gallon)
• Cabinet fitted with a thermostat controlled heater
• CAT5 AB Air gap to prevent backflow contamination
Dimensions (approx.) Electrical Approx Weight
Width: 610 mm Watts: 0.37 kW 30 kg
Depth: 390 mm Volts: 240 V
Height: 1070 mm Amps: 2.3 A
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