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The KGN Pillinger CAT 5 Washdown Booster Set is designed to prevent backflow contamination of the mains water supply, while maintaining flow and pressure. The unit is compact, lightweight, and housed in a stainless steel cabinet for easy wall mounting.

Advantages
· [image: ]Automatic operation
· Simple to wall or floor mount and install
· Easy access and maintenance
Design
Single diaphragm pump and water storage
tank house in a compact stainless steel cabinet                                                                                                                                     
1 outlet connection only

Applications 
· Bin store washdown
· Limited boosting applications
Features
· Standard stock item
· Illuminated ‘On/Off’ switch
· Duty: 0.25 l/s @ 2.2 bar (mid curve)
· Lightweight stainless steel cabinet
· Break Tank: 18 litre (4 gallon)
· Glycerine filled pressure gauge
· CAT5 AB Air gap to prevent backflow contamination
· Optional Extra: Cabinet can be fitted with a thermostat controlled heater 
Dimensions                          Electrical                                 Approx Weight
Width:  420 mm                     Watts:   0.37 kW                         25 kg                                                                                                                                                            Depth:  370 mm                     Volts:    240 V                                                                                                                                                                           Height: 750 mm                     Amps:   2.3 A     
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