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The KGN Pillinger Range of ‘Fill Spill’ units are designed for maintaining pressure on larger sealed systems and built with 304 stainless steel tanks for longevity.

Advantages
· Available in bespoke design builds to fit within plant room constraints
· Capable of temperatures  >120°C and extreme pressure changes
· Eliminates requirement for system expansion vessel
Design
Stainless steel tank connected to packaged booster set, comprising pump/s, control panel and expansion vessel on a single skid.

Applications

For use in larger heating systems where extreme pressure changes and high temperatures are likely.
· Commercial properties
· [image: ]Apartment buildings
· Leisure centres
· Industrial sites
· Water Utilities
· Office blocks
· Stadiums
· Hospitals
Features
· Multiple pumps configuration
· Multiple BMS volt free contacts
· Stainless steel base frame/skid
· 316L stainless steel pipework as standard
· Bespoke control panel for custom features and functions
· Bespoke stainless steel tank built to size with all connections
· Can be incorporated with other circulation and dosing equipment
· Inverter drive fitting available to achieve constant pressure control
· Remote telemetry system available to send fault signal alert via SMS text or telephone line
· Tank includes thermal spheres to reduce evaporation and assist in calming water at high temperature
· Anti-vibration mounts and flexible connections offered as standard to reduce noise throughout the building
· Can be supplied packaged with the tank on a common base fame or separate with interconnecting pipework between
 the tank and the pump set
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