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WashBoost® Compact AB

· Identical to the WashBoost® Compact, but includes a break tank providing Category 5 backflow protection via an AB Airgap. Where this unit is fed by the water main, the main is suitably protected from the serious health hazards present on wastewater sites. 
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