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WashBoost Compact 

· KGN Pillinger WashBoost® Compact is the most basic model available within this range. 
· Typical application is feeding manual washdown points on Water Utility Wastewater sites. 
· Off-site assembled packaged booster set on a fabricated 304 stainless-steel frame installed inside an IP55 enclosure with building services electrics. Requirement for a single power supply only.
· Fixed speed booster unit, pressure transducer controlled via a process controller with adjustable cut-in pressures – removing reliance away from unreliable pressure switches. Process controller forms part of an in-house assembled starter box. 
· All components are stocked parts, keeping lead times to a minimum. 
· Built to last, 304 stainless steel base frame, 316L stainless steel pipework, electrical components protected from a direct jet of water. High efficiency IE3 motor.
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