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WashBoost® Twin 

· A step up from the compact range, the WashBoost® Twin is a fully packaged, variable speed booster unit utilising “ultra-premium” synchronous motor and hydrovar® X+ inverter drives housed inside an enclosure, mounted on a heavy-duty stainless-steel skid.
· Configured Duty and Standby, the twin pump system provides resilience to the site wash water system. 
· Designed and manufactured with operators in mind; compact, yet maintainable. As the pump weights exceed manual handling limits, the kiosk design is tailored for the use of Reid Lifting equipment for removing a pump from the unit – ‘ALM’ friendly. 
· Form 2 local control panel, configured to meet the specific water authority specification requirements with our standard set of I/O’s including live delivery pressure readings available locally, and a 4-20mA signal to telemetry for remote monitoring. 
· 
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