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The KGN Pillinger range of KIWA (Regulation 4) approved AV & EV Booster Sets are designed and manufactured for use in a variety of applications including water distribution or pressure boosting where the existing water pressure is unable to meet the demand requirements.

Advantages
· Pump performance range extended by shared duty operation 
· Compact and bespoke design for custom fit installation
· [image: A black and white sign

Description automatically generated with low confidence]Variable speed for optimum running costs
Design
· Available in horizontal or vertical bespoke format
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EV:	Terminal box & Common volt free contacts (taken from inverters)     
AV:	Full control panel c/w individual volt free contacts 

Applications 
· Commercial properties
· Retail developments 
· Apartment blocks
· Water utilities
· Agricultural 
· Leisure centres
· Single dwellings
· Light industrial units
· Schools & universities
Features
· Stainless steel base frame
· Booster Sets available inside kiosks
· 316L stainless steel pipework as standard
· Individual motor mounted inverter drives on each pump
· Break tanks, filters and associated ancillary items available
· Single (EV) or Multiple (AV) BMS volt free contacts available
· Optional remote telemetry system to send fault signal alert via SMS text or telephone line
· Slow Fill system to prevent water surge following a power cut or if the unit cuts out due to low water level (AV)
· Anti-vibration mounts and flexible connections offered as standard to reduce noise transmission in the building
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