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WashBoost® Compact AB HR

· Identical to the WashBoost® Compact AB but includes a hose reel of varying lengths packaged inside the kiosk; 10, 20 and 30m lengths available. 
· Perfect for installation in areas with a local washdown requirement. 
· Spare discharge connection inside the kiosk for future requirements or for connection to a remote washdown area.  
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